<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.11-Bratislava">
  <identifier>GREG_SEAtribes</identifier>
  <parentidentifier></parentidentifier>
  <language>Eng</language>
  <type>dataset</type>
  <title>GREG_SEAtribes</title>
  <abstract>When using the GREG data for your research, please cite 
Weidmann, Nils B., Jan Ketil Rød, and Lars-Erik Cederman. 2010. "Representing Ethnic Groups in Space: A New Dataset". Journal of Peace Research 47(4): 491–99.
This file was extracted to cover only Southeast Asia, for the study of the Vietnam War.</abstract>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>Intelligence Military</keyword>
    <keyword>Society</keyword>
  </keywords>
  <contact>
    <name>mervyn roberts</name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>mervyn.roberts@ctcd.edu</email>
    <role></role>
  </contact>
  <links>
    <link format="" mimeType="" type="download" description="Geo-referencing of Ethnic Groups" name="undefined 1" size="" url="https://icr.ethz.ch/data/greg/"/>
    <link format="" mimeType="" type="" description="Representing Ethnic Groups in Space: A New Dataset" name="Weidmann, Nils B." size="" url="https://icr.ethz.ch/publications/representing-ethnic-groups-in-space/"/>
  </links>
  <dates/>
  <fees></fees>
  <constraints type="undefined 1">none</constraints>
  <rights></rights>
  <license>Creative Commons CC Zero</license>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>GEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],MEMBER["World Geodetic System 1984 (G2296)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],USAGE[SCOPE["Horizontal component of 3D system."],AREA["World."],BBOX[-90,-180,90,180]],ID["EPSG",4326]]</wkt>
      <proj4>+proj=longlat +datum=WGS84 +no_defs</proj4>
      <srsid>3452</srsid>
      <srid>4326</srid>
      <authid>EPSG:4326</authid>
      <description>WGS 84</description>
      <projectionacronym>longlat</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>true</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial miny="8.56366187999999973" minz="0" crs="EPSG:4326" maxx="109.44650821899999471" minx="100.08610045000000355" dimensions="2" maxz="0" maxy="23.39122595299999929"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
